{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":276,"n_cols":4,"rows_kept":276,"merged":[[5,0,5,1],[5,3,5,5],[5,8,5,10],[6,0,22,1],[6,3,6,5],[6,8,6,10],[7,3,7,5],[7,8,7,10],[8,3,8,5],[8,8,8,10],[9,3,9,5],[9,8,9,10],[10,3,10,5],[10,8,10,10],[11,3,11,5],[11,8,11,10],[12,3,12,5],[12,8,12,10],[13,3,13,5],[13,8,13,10],[14,3,14,5],[14,8,14,10],[15,3,15,5],[15,8,15,10],[16,3,16,5],[16,8,16,10],[17,3,17,5],[17,8,17,10],[18,3,18,5],[18,8,18,10],[19,3,19,5],[19,8,19,10],[20,3,20,5],[21,3,21,5],[22,3,22,5],[22,8,22,10],[23,0,28,1],[23,3,23,5],[23,8,23,10],[24,3,24,5],[25,3,25,5],[26,3,26,5],[27,3,27,5],[28,3,28,5],[29,0,36,1],[29,3,29,5],[30,3,30,5],[31,3,31,5],[32,3,32,5],[33,3,33,5],[34,3,34,5],[35,3,35,5],[36,3,36,5],[37,0,57,1],[37,3,37,5],[38,3,38,5],[39,3,39,5],[40,3,40,5],[41,3,41,5],[42,3,42,5],[43,3,43,5],[44,3,44,5],[45,3,45,5],[46,3,46,5],[47,3,47,5],[48,3,48,5],[49,3,49,5],[50,3,50,5],[51,3,51,5],[52,3,52,5],[53,3,53,5],[54,3,54,5],[55,3,55,5],[56,3,56,5],[57,3,57,5],[58,0,67,1],[58,3,58,5],[59,3,59,5],[60,3,60,5],[61,3,61,5],[62,3,62,5],[63,3,63,5],[64,3,64,5],[65,3,65,5],[66,3,66,5],[67,3,67,5],[68,0,68,5],[69,0,81,1],[69,3,69,5],[70,3,70,5],[71,3,71,5],[72,3,72,5],[73,3,73,5],[74,3,74,5],[75,3,75,5],[76,3,76,5],[77,3,77,5],[78,3,78,5],[79,3,79,5],[80,3,80,5],[81,3,81,5],[82,0,94,1],[82,3,82,5],[83,3,83,5],[84,3,84,5],[85,3,85,5],[86,3,86,5],[87,3,87,5],[88,3,88,5],[89,3,89,5],[90,3,90,5],[91,3,91,5],[92,3,92,5],[93,3,93,5],[94,3,94,5],[95,0,99,1],[95,3,95,5],[96,3,96,5],[97,3,97,5],[98,3,98,5],[99,3,99,5],[100,0,116,1],[100,3,100,5],[101,3,101,5],[102,3,102,5],[103,3,103,5],[104,3,104,5],[105,3,105,5],[106,3,106,5],[107,3,107,5],[108,3,108,5],[109,3,109,5],[110,3,110,5],[111,3,111,5],[112,3,112,5],[113,3,113,5],[114,3,114,5],[115,3,115,5],[116,3,116,5],[117,0,120,1],[117,3,117,5],[118,3,118,5],[119,3,119,5],[120,3,120,5],[121,0,129,1],[121,3,121,5],[122,3,122,5],[123,3,123,5],[124,3,124,5],[125,3,125,5],[126,3,126,5],[127,3,127,5],[128,3,128,5],[129,3,129,5],[130,0,141,1],[130,3,130,5],[131,3,131,5],[132,3,132,5],[133,3,133,5],[134,3,134,5],[135,3,135,5],[136,3,136,5],[137,3,137,5],[138,3,138,5],[139,3,139,5],[140,3,140,5],[141,3,141,5],[142,0,144,1],[142,3,142,5],[143,3,143,5],[144,3,144,5],[145,0,151,1],[145,3,145,5],[146,3,146,5],[147,3,147,5],[148,3,148,5],[149,3,149,5],[150,3,150,5],[151,3,151,5],[152,0,189,1],[152,2,152,5],[153,2,153,5],[154,2,154,5],[155,2,155,5],[156,2,156,5],[157,2,157,5],[158,2,158,5],[159,2,159,5],[160,2,160,5],[161,2,161,5],[162,2,162,5],[163,2,163,5],[164,2,164,5],[165,2,165,5],[166,2,166,5],[167,2,167,5],[168,2,168,5],[169,2,169,5],[170,2,170,5],[171,2,171,5],[172,2,172,5],[173,2,173,5],[174,2,174,5],[175,2,175,5],[176,2,176,5],[177,2,177,5],[178,2,178,5],[179,2,179,5],[180,2,180,5],[181,2,181,5],[182,2,182,5],[183,2,183,5],[184,2,184,5],[185,2,185,5],[186,2,186,5],[187,2,187,5],[189,2,189,5],[190,0,206,1],[190,2,190,5],[191,2,191,5],[192,2,192,5],[193,2,193,5],[194,2,194,5],[195,2,195,5],[196,2,196,5],[197,2,197,5],[198,2,198,5],[199,2,199,5],[200,2,200,5],[201,2,201,5],[202,2,202,5],[203,2,203,5],[204,2,204,5],[205,2,205,5],[206,2,206,5],[207,0,213,1],[207,2,207,5],[208,2,208,5],[209,2,209,5],[210,2,210,5],[211,2,211,5],[212,2,212,5],[213,2,213,5],[214,0,217,1],[214,2,214,5],[215,2,215,5],[216,2,216,5],[217,2,217,5],[218,0,218,5],[219,0,225,1],[219,2,219,5],[220,2,220,5],[221,2,221,5],[222,2,222,5],[223,2,223,5],[224,2,224,5],[225,2,225,5],[226,0,229,1],[226,2,226,5],[227,2,228,2],[227,3,227,5],[228,3,228,5],[228,6,228,8],[229,3,229,5],[230,0,250,1],[230,2,230,5],[231,2,231,5],[232,2,232,5],[233,2,233,5],[234,2,234,5],[235,2,235,5],[236,2,236,5],[237,2,237,5],[238,2,238,5],[239,2,239,5],[240,2,240,5],[241,2,241,5],[242,2,242,5],[243,2,243,5],[244,2,244,5],[245,2,245,5],[246,2,246,5],[247,2,247,5],[248,2,248,5],[249,2,249,5],[250,2,250,5],[251,0,251,5],[252,0,275,1],[252,2,252,5],[253,2,253,5],[254,2,254,5],[255,2,255,5],[256,2,256,5],[257,2,257,5],[258,2,258,5],[259,2,259,5],[260,2,260,5],[261,2,261,5],[262,2,262,5],[263,2,263,5],[264,2,264,5],[265,2,265,5],[266,2,266,5],[267,2,267,5],[268,2,268,5],[269,2,269,5],[270,2,270,5],[271,2,271,5],[272,2,272,5],[273,2,273,5],[274,2,274,5],[275,2,275,5]],"flags":["formulas_cached_only"]}
[]
[]
[]
[null,null,"产品目录"]
[]
["类型",null,"型号","功能说明"]
["电子蜡烛系列",null,"EC1068","正输出,蜡烛闪,闪烁幅度大,可以封装在LED内"]
[null,null,"EC1062A","负输出,蜡烛闪,有ON/OFF功能，闪烁幅度A款比较大可封装在LED内"]
[null,null,"EC1062B","负输出,蜡烛闪,有ON/OFF功能，闪烁幅度小（室内闪）,可以封装在LED内"]
[null,null,"EC1062C-01","正输出,蜡烛闪,闪烁幅度大,可以封装在LED内"]
[null,null,"EC1062C-02","负输出,蜡烛闪,输出电流大高亮度，幅度柔和,可以封装在LED内"]
[null,null,"EC1062C-03","负输出,蜡烛闪,高亮度幅度小,可以封装在LED内"]
[null,null,"EC1062C-04","负输出,蜡烛闪,高亮度幅度柔和,可以封装在LED内"]
[null,null,"EC1062C-05","负输出,蜡烛闪,高亮度幅度小,可以封装在LED内"]
[null,null,"EC1069B","负输出,单灯电子蜡烛IC,闪发新颖高亮度幅度轻柔有风吹渐变效果,可以封装在LED内"]
[null,null,"EC1066-C","声控蜡烛闪。可以吹亮灭,可蜂鸣片或咪头控制,外围电路简单。"]
[null,null,"EC1066-S","声控蜡烛闪，拍亮拍灭,蜂鸣片或咪头控制,外围电路简单。"]
[null,null,"EC1067-C","可吹亮灭声控IC,可蜂鸣片或咪头控制,外围电路简单，输出电平信号，可推LED灯或其他IC"]
[null,null,"EC1067-S","可拍亮拍灭声控IC,可蜂鸣片或咪头控制,外围电路简单，输出电平信号，可推LED灯或其他IC"]
[null,null,"EC1059","老版本蜡烛闪,两路输出,闪烁效果好.上电工作"]
[null,null,"EC1068BC","模拟致爱丽丝等音乐音乐蜡烛灯闪,"]
[null,null,"CF74/7178","红外人体感应蜡烛，当人体走近时候蜡烛亮，可保持亮，可做感应灯用"]
[null,null,"41C5","摇摆蜡烛，低电压启动，随机摇摆效果逼真。"]
["定时蜡烛系列",null,"EC340H-04","4/20,5/19,6/18,8/16,24/0,24小时定时循环,可选择定时或不定时,一路电平信号输出，晶体振荡"]
[null,null,"EC340A-D","4/20,6/18,7/17,8/16,24小时定时循环IC,两路输出,一路蜡烛闪,闪法改版,一路电平信号晶体振荡计时"]
[null,null,"EC1062-242C","4/20,5/19,6/18,8/16,24/0,24小时定时循环IC,可选择定时或不定时,两路输出,一路蜡烛闪一路电平,晶体振荡"]
[null,null,"EC1062-242C","4/20,5/19,6/18,8/16,24/0,24小时定时循环IC,可选择定时或不定时,两路输出,一路蜡烛闪一路电平,晶体振荡"]
[null,null,"EC360A-01","4/20,5/19,6/18,8/16,24/0,24小时定时循环IC,可选定时或不定时,6路输出,5路蜡烛闪，一路电平输出晶体振荡"]
[null,null,"EC360A-02","4/20,5/19,6/18,8/16,24/0,24小时循环,可选择定时或不定时,6路输出,3路顺闪3路多彩渐变晶体振荡,可做灯串"]
["红外线遥控蜡烛",null,"ECR08B","红外线遥控蜡烛,两个按键,一个ON,一个OFF,遥控器采用通用的IC,EC6122"]
[null,null,"EC209B","红外线遥控定时蜡烛,10个按键,4/20,5/19,8/16,24小时循环定时,或选择不循环,遥控器采用通用的IC,EC6122"]
[null,null,"EC607","18按键遥控蜡烛，遥控功能有ON/OFF，七彩闪，RGB，可调各种颜色，有4/8H循环定时。遥控采用6122"]
[null,null,"EC1062BR","7按键遥控定时蜡烛，遥控功能有ON，OFF，6H，4H，5H，8H ，24小时循环"]
[null,null,"ECR06A","2按键红外遥控，ON/OFF开关功能。"]
[null,null,"EC69D4","12按键遥控定时，有2/22,4/20,5/19,10/14循环定时，有light和candle功能，加减按键可遥控调亮度，"]
[null,null,"EC1062CR","7按键遥控定时蜡烛，遥控功能有ON，OFF，6H，4H，5H，8H ，24小时循环"]
[null,null,"ECR09","省电模式,红外线遥控蜡烛,两个按键,一个ON,一个OFF,采用低功耗技术，可以节省90%电(接收头功耗),"]
["定时IC系列",null,"EC340A","10秒,5分,30分,1H,2H,4H,8H,10H,定时,ON/OFF或OS控制,中途触发可以重新计时,可以选择晶振或RC振荡,"]
[null,null,"EC340B","8/16小时定时IC,晶体振荡计时"]
[null,null,"EC340C","上电工作，9秒-40分时间可调，，RC振荡计时。"]
[null,null,"EC340D","上电不工作，定时6秒-10分钟，中途触发会停止掉。"]
[null,null,"EC340E-02","上电不工作,触发功能,中途触发无效15秒--30分钟时间可调,RC振荡,简易定时IC"]
[null,null,"EC340E-01B","上电不工作,触发功能,中途触发无效15秒内时间可调,RC振荡,简易定时IC"]
[null,null,"EC026-082","定时1小时芯片，ON/OFF功能，可做定时器用，4路输出，1路电平信号输出，3路渐变输出，也可选择一种颜色"]
[null,null,"EC340EGON","上电不工作,触发功能,中途触发无效15秒--50小时，时间可调,RC振荡,简易定时IC"]
[null,null,"EC340H-04","2/22,3/21,4/20,5/19,6/18,8/16,10/14,24小时循环定时,晶体振荡,设计外围电路简单功能多成本低"]
[null,null,"EC24H","定时IC，触发开关可编程定时时间，1-24小时循环，"]
[null,null,"EC340A-D","4/20,6/18,7/17,8/16,24小时定时循环IC,两路输出,一路蜡烛闪,有电平信号输出，晶体振荡计时"]
[null,null,"ECH1062-242C","4/20,5/19,6/18,8/16,24/0,24小时定时循环IC,可选择定时或不定时,两路输出,一路蜡烛闪一路电平,晶体振荡"]
[null,null,"ECH1062-242D","4/20,5/19,6/18,8/16,24/0,24小时定时循环IC,可选择定时或不定时,两路输出,一路蜡烛闪一路电平,晶体振荡"]
[null,null,"EC360A-01","4/20,5/19,6/18,8/16,24/0,24小时定时循环IC,可选定时或不定时,6路输出,5路蜡烛闪，一路电平输出晶体振荡"]
[null,null,"EC360A-02","4/20,5/19,6/18,8/16,24/0,24小时循环,可选择定时或不定时,6路输出,3路顺闪3路多彩渐变晶体振荡,可做灯串"]
[null,null,"EC209B","遥控定时带蜡烛闪,10个按键,4/20,5/19,8/16,24小时循环定时,或选择不循环,遥控器采用通用的IC,EC6122"]
[null,null,"EC607","18按键遥控带定时，遥控功能有ON/OFF，七彩闪，RGB，可调各种颜色，有4/8H循环定时。遥控采用6122"]
[null,null,"EC1062BR","7按键遥控带定时，遥控功能有ON，OFF，6H，4H，5H，8H ，24小时循环"]
[null,null,"EC69D4","12按键遥控定时，有2/22,4/20,5/19,10/14循环定时，有light和candle功能，加减按键可遥控调亮度，"]
[null,null,"EC1062CR","7按键遥控带定时，遥控功能有ON，OFF，6H，4H，5H，8H ，24小时循环"]
[null,null,"EC4331","倒计时，正计时。4位液晶显示，倒计时：59分59秒或99分59秒，有报警提示功能"]
["开关OR手电筒IC",null,"EC3201B","上电不工作,触发亮-灭,电平信号输出,可以做ON/OFF开关用,高压工艺,可以使用6V"]
[null,null,"EC6A-01","上电不工作,触发闪-亮-灭。可选择闪烁速度2HZ或4HZ,输出电流大,高压工艺,可以使用6V"]
[null,null,"EC6A-02","触发依次亮--慢闪-快闪-灭,可以选择快闪和慢闪不同方式,输出电流大,高压工艺,可以使用6V"]
[null,null,"EC6A-03","触发依次,亮--闪-灭,可以选择快闪和慢闪不同方式,输出电流大,高压工艺,可以使用6V"]
[null,null,"EC6A-04","触发依次50%亮--100%亮-灭,可选择50%或100%的先后方式,输出电流大,高压工艺,可以使用6V"]
[null,null,"EC6A-05","上电不工作，触发下亮，触发下灭，电平输出，可做开关用，可选有SOS功能，输出电流大,高压工艺,可以使用6V"]
[null,null,"EC6A-B","上电不工作，触发依次为亮--爆闪（10HZ）--灭，可选有SOS功能，输出电流大,高压工艺,可以使用6V"]
[null,null,"ECY01","1-3W/LED手电筒驱动IC，SOT23封装，全亮-半亮-爆闪，过热电池反装开路短路保护"]
[null,null,"ECY02","3-5W/LED手电筒驱动IC，SOT23封装，全亮-半亮-爆闪，拨动开关选择输出模式"]
[null,null,"ECY05","3-5W/LED手电筒驱动IC，SOT23封装，全亮-半亮-微亮-爆闪-SOS功能，拨动开关选择输出模式"]
["闪灯IC系列"]
["1灯",null,"EC6A-01","上电不工作,触发闪-亮-灭。可选择闪烁速度2HZ或4HZ,输出电流大,高压工艺,可以使用6V"]
[null,null,"EC6A-02","触发依次亮--慢闪-快闪-灭,可以选择快闪和慢闪不同方式,输出电流大,高压工艺,可以使用6V"]
[null,null,"EC6A-03","触发依次,亮--闪-灭,可以选择快闪和慢闪不同方式,输出电流大,高压工艺,可以使用6V"]
[null,null,"EC6A-04","触发依次50%亮--100%亮-灭,可选择50%或100%的先后方式,输出电流大,高压工艺,可以使用6V"]
[null,null,"EC6A-05","上电不工作，触发下亮，触发下灭，电平输出，可做开关用，可选有SOS功能，输出电流大,高压工艺,可以使用6V"]
[null,null,"EC105C-01","亮-闪(3.8Hz)-灭"]
[null,null,"EC105C-02","亮-闪--灭"]
[null,null,"EC105C-03","快闪(6Hz)-慢闪(3Hz)-亮-灭"]
[null,null,"EC106-128-24","触发闪128圈,2.4HZ"]
[null,null,"EC106-24","上电工作,ON/OFF,2.4HZ"]
[null,null,"EC106C-06","上电工作,ON/OFF,0.6HZ,闪亮的占空比不同"]
[null,null,"EC610-24-06","单灯1路输出，ON/OFF功能，1/8,1/32DUTY,2.4HZ,0.6HZ"]
[null,null,"EC106-06","上电工作,ON/OFF,0.6HZ"]
["两灯",null,"EC5601","亮--闪--爆闪--灭,"]
[null,null,"EC5B06","触发功能，爆炸闪，快闪，全亮（快闪），灭。两路输出同步。"]
[null,null,"EC5B16","触发功能，闪、全亮（快闪）、灭。两路输出同步。"]
[null,null,"EC5B26","触发功能，快闪、慢闪、全亮（快闪）、灭。两路输出同步。"]
[null,null,"EC5B36","触发功能，全亮（快闪）、闪、灭。两路输出同步。"]
[null,null,"EC5B16-02","触发功能，闪、全亮、灭。两路输出同步。"]
[null,null,"EC5B36B-25","触发功能，爆闪--闪--亮--灭,高电压设计,大电流输出。两路输出同步。"]
[null,null,"EC342B","2灯对闪1/2DUTY  1.5HZ"]
[null,null,"EC109-B","跳闪--齐闪--亮--灭"]
[null,null,"EC109-C","亮---闪--灭"]
[null,null,"EC109-D","100%亮--30%亮--闪--灭,"]
[null,null,"EC109-E","30%亮--100%亮--闪--灭"]
[null,null,"EC109-F","亮--快闪---慢闪--灭"]
["两灯",null,"EC2022","对闪,2.0HZ,1/2DUTY"]
[null,null,"EC2026","对闪,2.6HZ,1/2DUTY"]
[null,null,"EC1622","触发抖动32圈约15秒自动停，约2.0HZ,"]
[null,null,"EC1202B","L1亮--L1L2亮---灭"]
[null,null,"EC1202C","L1亮--L2亮---灭"]
["三灯",null,"EC3L-30","3灯上电顺闪，ON/OFF,1/6DUTY,3.0HZ"]
[null,null,"EC3LH-35","3灯上电顺闪，ON/OFF功能，1/6DUTY。3.5HZ"]
[null,null,"EC3LF-68","3灯上电顺闪，ON/OFF功能，1/6DUTY,6.8HZ"]
[null,null,"EC3LH-68","3灯上电顺闪，ON/OFF功能，1/6DUTY"]
[null,null,"EC1246","三灯七彩7段闪（顺闪-渐明渐暗-全亮-红闪-绿闪-蓝闪-灭）"]
[null,null,"EC3300C","上电闪3灯渐明渐暗，ON/OFF,1/2PHASE"]
[null,null,"EC3301-01/02/03","3灯渐明渐暗，多种闪法选择，可光控，ON/OFF,上电闪，或触发闪一段时间自动停"]
[null,null,"EC3302-12/13","上电3灯渐明渐暗，触发多段闪"]
[null,null,"EC3179B","3灯渐明渐暗，多种闪法选择，可光控，ON/OFF,上电闪。"]
[null,null,"EC3301C","3灯渐明渐暗，多种闪法选择，可光控，ON/OFF,上电闪，或触发闪一段时间自动停"]
[null,null,"EC2095B-32","3LED多彩上电连续变化，ON/OFF功能和OSH-4功能（4圈），3LED90°变化"]
[null,null,"EC2095C","3LED多彩连续变化，上电不闪，LH功能用于CDS"]
[null,null,"EC3049系列","3灯渐明渐暗，多段闪，ON/OFF,OS功能，上电闪，"]
[null,null,"EC1233系列","3灯渐明渐暗，多段闪，ON/OFF,OS功能，上电闪，"]
[null,null,"EC1236","3灯渐明渐暗，内置在LED中，正输出"]
[null,null,"EC1233DRH-05/12","用于鞋灯，3灯七彩闪，触发功能"]
[null,null,"EC1233R-5/12","用于打火机，3灯七彩闪，触发功能"]
["4灯",null,"CDT3143A","上电工作4灯渐明渐暗,可光控，外接振荡电阻。"]
[null,null,"CDT3143","上电工作4灯渐明渐暗,可光控，外接振荡电阻"]
[null,null,"EC3143B","上电工作4灯渐明渐暗,可光控，外接振荡电阻"]
[null,null,"EC3407A-02","上电工作，有ON/off带暂停功能，常用于小夜灯"]
["5灯",null,"EC3335","5灯触发，来回闪，顺闪---全闪---全亮--灭"]
[null,null,"EC3338","5灯8段，触发功能：全亮；全闪、慢全闪、顺闪、逆闪、快顺闪、来回闪、灭。"]
[null,null,"EC3339","5灯8段可触发可连续工作：单灯来回闪，双灯来回闪，连亮，连灭，由外向内来回闪， 全闪，连亮连灭，渐明渐暗"]
[null,null,"EC666B","5灯带图案旋转陀螺"]
[null,null,"EC1566","5灯触发闪4/8/16/32圈，2.6HZ"]
[null,null,"EC2096系列","5灯触发闪2/4/8/16/32圈，2.6HZ部分可耐高电压工艺，主要用鞋灯火打火机"]
[null,null,"EC3369","5灯8段闪；上电自动循环8段闪，或触发分段闪,可外调闪烁速度。"]
[null,null,"EC2093","5LED，4功能闪，顺闪、来回闪、同时闪、停"]
[null,null,"EC1027-06","手电筒头灯IC,5灯多功能，16种模式多段闪烁"]
["6灯",null,"EC1836A-01/02/03/04","6灯顺闪，触发闪32/16/8/4圈"]
[null,null,"EC1660A-01-02-03","6闪灯，可顺闪，来回闪，ON/OFF，OS触发闪16周功能，频率可调"]
[null,null,"EC1611-01-02","6灯顺闪，可乱闪，触发闪16圈，可光控"]
[null,null,"EC1660C-01","6灯顺闪、来回闪；ON/OFF、OSH、LH；1/12duty；高电压设计6.8V"]
[null,null,"EC1660C-02/03/04","6灯顺闪、来回闪；ON/OFF、OSH、LH；1/12duty；1.0/1.5/2.0/3.0Hz"]
[null,null,"EC3245B","6灯 顺闪，外接振荡电阻，ON/OFF；OS闪16圈"]
[null,null,"EC2090AB","6灯，顺闪，ON/OFF功能，1/6DUTY,2.4HZ,3.6HZ,4.0HZ，7.0HZ"]
[null,null,"EC625","6灯上电顺闪，ON/OFF功能，1/6DUTY,1.0/1.5/2.4/3.0/6.8HZ"]
[null,null,"EC1656","6灯上电顺闪，1.5,2.4，3.0，6.8HZ"]
[null,null,"EC1070","上电不闪 6灯顺闪ON/OFF功能，也选择OS触发功能32周，可随意调整闪烁速度，"]
[null,null,"EC1071","上电闪 6灯顺闪ON/OFF功能，也选择OS触发功能32周，可随意调整闪烁速度，"]
[null,null,"EC688","赌博机，6LED触发随机停，有声音输出。"]
["7灯-10灯",null,"EC672","7灯顺闪，OS触发、ON/OFF开关功能，有16/32圈选择，1/7Duty"]
[null,null,"EC818","8灯顺闪，ON/OFF功能，外置振荡"]
[null,null,"EC7350","十闪灯,汽车灯,可用12V,顺闪,全亮,同时闪,来回闪,连亮"]
["圣诞灯串系列",null,"EC80058","4路8段输出,LED灯串，可上电自动变换各段,也可按键触发选择各段,有渐明渐暗功能，有DICE和SOP-8封装"]
[null,null,"EC826","太阳能光控功能，有定时功能，2路2线8段输出,可上电自动变换各段,也可按键触发选择各段."]
[null,null,"EC263C","4路多段输出,2按键选择6-16段及闪烁速度."]
[null,null,"EC263M","4路8段输出,可上电自动变换各段,也可按键触发选择各段,有渐明渐暗功能,有记忆功能"]
[null,null,"EC263-1","4路6段调速,按键触发调速"]
[null,null,"EC273","10路8段功能,旋转开关选择各段功能"]
[null,null,"EC273C","4/2路输出,按键开关选择8段功能,有渐明渐暗功能"]
["单音音乐",null,"EC5230B系列      触发功能推LED"]
[null,null,"EC5230B-01  生日歌，触发开关，工作一段时间自动停止，推LED"]
[null,null,"EC5230B-02  小星星，触发开关，工作一段时间自动停止，推LED"]
[null,null,"EC5230B-03 圣诞三曲，触发开关，工作一段时间自动停止，推LED"]
[null,null,"EC5230B-05  爱情故事，触发开关，工作一段时间自动停止，推LED"]
[null,null,"EC5230B-06 小小世界，触发开关，工作一段时间自动停止，推LED"]
[null,null,"EC5230B-07  甜蜜的家，触发开关，工作一段时间自动停止，推LED"]
[null,null,"EC5230B-08  玛丽有个小绵羊，触发开关，工作一段时间自动停止，推LED"]
[null,null,"EC5230B-09  致爱丽丝， 触发开关，工作一段时间自动停止，推LED"]
[null,null,"EC5230B-10  婚礼进行曲，触发开关，工作一段时间自动停止，推LED"]
[null,null,"EC5230B-11  温柔的爱，触发开关，工作一段时间自动停止，推LED"]
[null,null,"EC5230B-12  祝您圣诞快乐，触发开关，工作一段时间自动停止，推LED"]
[null,null,"EC5230B-13  圣诞铃声， 触发开关，工作一段时间自动停止，推LED"]
[null,null,"EC5230B-14  平安夜，触发开关，工作一段时间自动停止，推LED"]
[null,null,"EC5230B-15  您是我阳光，触发开关，工作一段时间自动停止，推LED"]
[null,null,"EC5230B-16  让我叫你小甜心，触发开关，工作一段时间自动停止，推LED"]
[null,null,"EC5230B-22  摇篮曲，催眠曲，触发开关，工作一段时间自动停止，推LED"]
[null,null,"EC5230B-32门铃声"]
[null,null,"EC5230L系列         上电长响  "]
[null,null,"EC5230L-01  生日歌，上电循环工作，推LED"]
[null,null,"EC5230L-02  小星星，上电循环工作，推LED"]
[null,null,"EC5230L-03  圣诞三曲，上电循环工作，推LED"]
[null,null,"EC5230L-05  爱情故事，上电循环工作，推LED"]
[null,null,"EC5230L-06  小小世界，上电循环工作，推LED"]
[null,null,"EC5230L-07  甜蜜的家，上电循环工作，推LED"]
[null,null,"EC5230L-08  玛丽有个小绵羊，上电循环工作，推LED"]
[null,null,"EC5230L-09   致爱丽丝，上电循环工作，推LED"]
[null,null,"EC5230L-10  婚礼进行曲，上电循环工作，推LED"]
[null,null,"EC5230L-11   温柔的爱，上电循环工作，推LED"]
[null,null,"EC5230L-12  祝您圣诞快乐，上电循环工作，推LED"]
[null,null,"EC5230C-13  圣诞铃声，上电循环工作，推LED"]
[null,null,"EC5230L-14  平安夜,上电循环工作，推LED"]
[null,null,"EC5230L-15  您是我阳光,上电循环工作，推LED"]
[null,null,"EC5230L-16  让我叫你小甜心,上电循环工作，推LED"]
[null,null,"EC5230L-22  摇篮曲，催眠曲,上电循环工作，推LED"]
[null,null,"EC5230L-35  人生佳年华,上电循环工作，推LED"]
[null,null,"EC5230D-001C  生日歌，低压适用1.5V纽扣电池，上电循环播放，无LED"]
[null,null,"EC5238L-001  生日歌，低压适用1.5V纽扣电池推蜂鸣器或喇叭，上电循环播放，无LED"]
["其他音乐IC",null,"其他音乐IC"]
[null,null,"EC312A-01  儿歌三首,触发功能,推LED,128音符 "]
[null,null,"EC312A-03  圣诞三首,触发功能,推LED,128音符"]
[null,null,"EC5232-01  儿歌12首打点,触发功能,推4LED顺闪,双音"]
[null,null,"EC5232-04  儿歌12首,触发功能,推4LED顺闪,双音"]
[null,null,"EC5232-06  圣诞10首,触发功能,推4LED顺闪,双音"]
[null,null,"EC3308       和弦声圣诞音乐8首,推七彩灯闪烁"]
[null,null,"EC3309-11  和弦声儿歌音乐16首,推4LED,有随音频闪,有3LED七彩灯闪烁,可推马达"]
[null,null,"EC3309-12  和弦声圣诞音乐12首,推4LED,有随音频闪,有3LED七彩灯闪烁,可推马达"]
[null,null,"音效IC"]
[null,null,"EC3210-01   飞机声,摩托车声,机枪声,推LED"]
[null,null,"EC306D      报警声IC，单声报警，可触发或长响"]
[null,null,"EC9310      鬼叫声,可长响或触发功能,推LED"]
[null,null,"EC305      消防车,救护车,警车声,机器声,可长响或触发功能,推LED"]
[null,null,"EC5239     八声三闪,枪声,马达声,电话铃声等,推3 LED闪烁."]
[null,null,"EC2381-02   音乐玩具电话,自动拨号声,电话铃,忙音,音乐声等"]
[null,null,"EC2386-01  俄文玩具电话,俄文儿童语音,电话铃声等"]
["电源稳压及升压",null,"EC6206     输出 DC3.0V,DC3.3V,DC3.6V,DC4.5V,低压稳压电路"]
[null,null,"EC6208     输入电压最高DC16V，输出3.0V,3.3V, 3.6V等，  89-3,23-3封装"]
[null,null,"EC2002     降压恒流驱动，输入电压DC6V-55V，恒流输出可达1.2A，输出可调。"]
[null,null,"ECHXX      DC/DC升压转芯片，内置二极管，3.3V,3.6V输出,SOT-23-3封装，成本低。"]
[null,null,"ECH601     LED升压IC，主要针对手电筒产品或负载输出端升压，通过电感调节电流，简单成本低"]
[null,null,"EC1002   同步升压IC，DC/DC，内置二极管，多种输出电压值可选择"]
[null,null,"EC0828    DC/DC升压IC外置二极管，输出电压多种选择。"]
["触摸IC及方案",null,"EC022S    两通道两输出触摸控制IC，可选高低电位输出，抗干扰能力强，SOP-8封装"]
[null,null,"EC022W    单通道LED灯触摸芯片，无级或3段调整亮度抗干扰性好"]
[null,null,"EC022K    两通道两输出触摸芯片，可选高低电位输出，可LH保持输出信号（长按长亮）"]
[null,null,"EC023W    单通道两输出触摸控制，亮度可随意控制可分段"]
["录音IC"]
["录音IC",null,"EC1806B,   6秒录音IC，掉电保存资料，触发开关录放音，LED指示，有音乐声"]
[null,null,"ISD1806X   6-10录音IC，高清晰音质，可掉电保存"]
[null,null,"ISD1810X   8-16秒录音IC，高清晰音质，可掉电保存"]
[null,null,"ISD1616X   10-30秒录音IC，高清晰音质，可掉电保存"]
[null,null,"AMSRB006A   6秒录音IC，触发开关录放音，"]
[null,null,"AMSRC010A   10秒录音IC，触发开关录放音，"]
[null,null,"EC200      30秒以上录音IC，外加FLASH"]
["语音IC",null,"语音IC,"]
[null,null,"EC036-XX系列","猪叫，牛叫，马叫，羊叫，狮子，大象，老虎，青蛙，猴子，狗叫，猫叫，母鸡公鸡叫声等等"]
[{"$nulls":3},"各类汽车声，火车声，枪声，电话声，小孩笑声，巫婆笑声，哭声"]
[null,null,"EC016-XX系列","圣诞节歌曲，儿歌歌曲，情歌歌曲：圣诞快乐，男女声圣诞，圣诞老公公进城，你是我的阳光，摇篮曲，小星星等"]
["其他电路",null,"其他电路IC"]
[null,null,"EC3010       红外遥控电路，外接三极管"]
[null,null,"EC6122       红外遥控标准版，全编码，省三极管，省电容"]
[null,null,"EC9122       普通遥控器，省电容，外接三极管"]
[null,null,"ECD9122X     可内置编码9122摇控器"]
[null,null,"EC688        赌博机，6LED触发随机停，固定位置音效输出"]
[null,null,"EC408        声控音效IC，小鸟叫，输出推喇叭，接收用蜂鸣片"]
[null,null,"EC28         四种声音: 小鳥叫 ,單音樂 ,電話鈴聲 ,二隻老虎."]
[null,null,"EC2011       带波包单音门铃－2声"]
[null,null,"EC2011B      带波包单音门铃－3声"]
[null,null,"EC313A       直升机马达＋枪声"]
[null,null,"ECD4331       LCD定时，倒计时"]
[null,null,"ECD801-16     太阳能LCD闪－1.6Hz"]
[null,null,"ECD801-0.8    太阳能LCD闪－1.0Hz"]
[null,null,"ECD801-0.5    太阳能LCD闪－0.5Hz"]
[null,null,"ECS5096-33    电源管理降压恒压输出3.3V"]
[null,null,"ECD1001       雪花灯内置LED"]
[null,null,"ECD1002       雪花灯串控制IC"]
[null,null,"ECD716C-3     口哨BI.BI.BI，低频率"]
[null,null,"ECP-8488      乱弹琴"]
[null,null,"GC28          四种声音：小鳥叫，單音樂，電話鈴聲，二隻老虎"]
["通用标准品IC"]
["通用标准品",null,"TDA2822M     双声道功放电路  "]
[null,null,"TDA2003V      10W单功放电路    "]
[null,null,"TA2003P          AM/FM收音电路      "]
[null,null,"TEA2025         立体音频双功放电话        "]
[null,null,"TDA2030A      18W双功放电路    "]
[null,null,"EC0030              1.5W输出功率的模拟音频功率放大器,外围电路简单       "]
[null,null,"EC4871A/B      音频功放IC，用于MP3、PDA等音频放大器，SOP-8"]
[null,null,"LM386            低功耗音频放大电路            "]
[null,null,"L7805/7805     3端0.1A正电源稳压电路           "]
[null,null,"78L08              3端0.1A正电源稳压电路            "]
[null,null,"78L12               3端0.1A正电源稳压电路               "]
[null,null,"LM393           双电压比较器集成电路。"]
[null,null,"LM358           双重运算放大器"]
[null,null,"NE555            时基电路          "]
[null,null,"LM431          精密电压基准源"]
[null,null,"EC1621SS       128点LCD驱动器,裸片"]
[null,null,"EC1622           32×8位 LCD驱动IC，256点LCD显示"]
[null,null,"EC2301           20V P沟道增强型MOS场效应管，电源管理、小功率驱动等，SOT23-3"]
[null,null,"EC2302          20V N沟道增强型MOS场效应管，电源管理、小功率驱动等，SOT23-3"]
[null,null,"AT24C02      存储器IC"]
[null,null,"C9389           8位计算器IC"]
[null,null,"EC8072         变音IC"]
[null,null,"SN2501       单片机"]
[null,null,"SN2711     单片机"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}